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Spring drilling: AEROSEM in constant use 
Perfect seed germination in all cultures 
Thanks to the successful integration of precision seed drilling technology into a standard pneumatic seed drill, the Pöttinger AEROSEM offers the highest operational flexibility and is in continuous operation during the spring planting season. Working with maize today, soya tomorrow and cereals on day three - the Pöttinger AEROSEM makes it possible. This is something that is much appreciated and brings a great deal of satisfaction to the professionals using this machine. Arable farmers are impressed at how well and how easily the system works and in addition to the advantages of being able to handle such a wide range of crops, can also confirm perfect seed germination. 
 
PCS and IDS: Multiple international award-winning technology

a) PCS (Precision Combi Seeding) 
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]The drill is fitted with up to ten precision coulters for a row spacing of 37.5 cm or 75 cm, or only 12.5 cm on the AEROSEM ADD. Using the standard metering system with a distributor head add-on, fertilizer can be applied between the seed rows. Grass seed can also be drilled simultaneously, combined with individual seed drilling, to provide optimum erosion protection. With DUPLEX SEED, silage and corn maize is planted in double rows. In addition to increasing yield, it also increases output during drilling thanks to the higher driving speed. As a result, DUPLEX SEED is a real economical alternative to conventional precision seed drilling.

b) IDS (Intelligent Distributor System):
IDS is a unique system worldwide that guarantees a consistent flow of seed to each row, saving seed material usage. The unique distributor head with integrated double-wall tube system for internal grain return on tramlines is a guarantee that with cereals and small seeds the cross distribution values can be precisely measured - especially in the rows next to the tramlines - to ensure that seed density stays constant. 

A great number of perfect coulter systems guarantee exact placement oft he seed. The machine is available with 3 rows of Suffolk coulters, a single row or with DUAL DISC double-disc coulters. The Suffolk coulters are suitable for light soil with low levels of organic matter. A coulter pressure of up to 55 lbs / 25 kg can be applied to Suffolk coulters and single-disc coulters. The large DUAL DISC coulters cut right through surface trash to form a uniform, tidy furrow 
Depending on the type of seed, the metering wheels can be exchanged quickly and easily. 

Die AEROSEM spielt ihr Potenzial voll aus mit einer LION Kreiselegge, einer FOX Kurzkombination zur Saatbettbereitung oder dem neuartigen Konzept der MULTILINE, das eine Kurzscheibenegge oder einen Grubber mit der Sämaschine vereint.

One drill for all crops: regardless of which crops are due to be sown this spring, the Pöttinger AEROSEM guarantees the highest operating flexibility, precision and convenience in one machine. Precisely the right kit for every arable professional. 
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AEROSEM 3002 ADD
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